Survey

Ip survey are using the same setup as DC resistivity survey. Both surveys are acquired togther. Only the measurements change as induced polarization survey use off-time measurements whereas DC resistivity survey use on-time measurements.

See the section dc\_surveys for more information.