Rock Chageability for Various Minerals

This table shows the approximate integrated chargeabilities for 1 % content of various minerals. The values below were obtained by integrating from 0.02 - 1.0 seconds.

| **Mineral Type** | **Chargeability (msec)** |
| --- | --- |
| pyrite | 13.4 |
| chalcocite | 13.2 |
| copper | 12.3 |
| graphite | 11.2 |
| chalcopyrite | 9.4 |
| bornite | 6.3 |
| galena | 3.7 |
| magnetite | 2.2 |
| malachite | 0.2 |
| hematite | 0.0 |