Rock Chageability for Various Rocks

This table shows the approximate integrated chargeabilities for various rocks. The values below were obtained by integrating from 0.02 - 1.0 seconds.

| **Material type** | **Chargeability (msec)** |
| --- | --- |
| ground water | 0 |
| alluvium | 1-4 |
| gravels | 3-9 |
| precambrian volcanics | 8-20 |
| precambrian gneisses | 6-30 |
| schists | 5-20 |
| sandstones | 3-12 |
| argilites | 3-10 |
| quartzites | 5-12 |